Bobrick offers over 750 products for public washroom facilities and five series of toilet partitions. If you are not familiar with the Bobrick product line, please view the Full Catalog at [www.bobrick.com](http://bobrick.com/productsupport/Pages/LiteratureSupport.aspx) or contact your local representative for assistance, by calling 818-503-1600 or by [searching on our website](http://bobrick.com/Pages/RepresentativeAndDistributorFinder.aspxhttp%3A/bobrick.com/Pages/RepresentativeAndDistributorFinder.aspx) by state or country.

This specification section is provided in CSI-format and intended to be included in the Project Manual for a construction project. Delete models and options not required for your project and modify to your project requirements. © 1966-2021 Bobrick Washroom Equipment, Inc.

SECTION 102800

WASHROOM ACCESSORIES

1. GENERAL
	1. SECTION INCLUDES
		1. Washroom accessories as scheduled in this Section and as indicated on the Drawings.
	2. RELATED REQUIREMENTS
		1. Section 061000 - Rough Carpentry, coordination with blocking.
		2. Section 092000 - Plaster and Gypsum Board, coordination with blocking.
		3. Section 093000 - Tiling, coordination with layout and installation.
		4. Section 102113 - Toilet Compartments, coordination with accessories.
		5. Section 102814 - Baby Changing Stations, for baby changing stations.
	3. SUBMITTALS
		1. Product Data: Submit manufacturer's data sheets for each product specified, including the following:
			1. Installation instructions and recommendations.
			2. Storage and handling requirements and recommendations.
			3. Cleaning and maintenance instructions.
			4. Replacement parts information.
		2. Schedule: Submit a toilet accessory schedule, indicating the type and quantity to be installed in each washroom. Use room numbers as indicated on the Drawings.
		3. USGBC LEED Submittals, Recycled Content: Materials and Resource Credits MR4.1 and MR4.2 - Recycled Content: Submit manufacturer’s calculation of value of recycled content for specified products, calculated in accordance with USGBC LEED certification requirements.
		4. Country of Origin: Manufacturer must supply, with first submittal, Country of Origin information for each type of washroom accessory for this project.
	4. QUALITY ASSURANCE
		1. Manufacturer: Provide products manufactured by a company with a minimum of 10 years successful experience manufacturing similar products.
		2. Single Source Requirements: To the greatest extent possible provide products from a single manufacturer.
		3. Accessibility Requirements: Comply with requirements applicable in the jurisdiction of the project, including but not limited to ADA and ICC/ANSI A117.1 requirement as applicable.
		4. Hazardous Materials: Comply with EU Directive “Restrictions of Hazardous Substances (RoHS) requirements.”
	5. DELIVERY, STORAGE, AND HANDLING
		1. Deliver, store and handle materials and products in strict compliance with manufacturer's instructions and recommendations. Protect from damage.
	6. WARRANTY
		1. Manufacturer’s Warranty for Washroom Accessories: Manufacturer’s standard 1 year warranty for materials and workmanship.
		2. Manufacturer’s Warranty for Electric Hand Dryers: Manufacturer’s standard 5-year warranty on parts, except 3 year warranty on motor brushes from date of purchase.
2. PRODUCTS
	1. MANUFACTURER
		1. Basis of Design Products: Based on the quality and performance requirements of the project, specifications are based solely on the products of Bobrick Washroom Equipment, Inc.. [www.bobrick.com](http://www.bobrick.com). Location of manufacturing shall be the United States.
		2. Substitutions: The Architect will consider products of comparable manufacturers as a substitution, pending the contractor's submission of adequate documentation of the substitution in accordance with procedures in Division 1 of the Project Manual. Documentation shall include a list of five similar projects of equivalent size where products have been installed for a minimum of two years, and manufacturer's certification that products are fabricated in the United States.
	2. TOILET ACCESSORY SCHEDULE
		1. Single-User Washroom, Standard Duty:
			1. TA-1: B-5806 Series Concealed Mounting Grab Bar – 1-1/4 inch diameter.
			2. TA-2: B-165 Series Channel-Frame Mirror.
			3. TA-3: B-2888 ClassicSeries Surface-Mounted Multi-Roll Toilet Tissue Dispenser.
			4. TA-4: B-3944 ClassicSeries Recessed Paper Towel Dispenser / Waste Receptacle with 3944-130 TowelMate Accessory and 3944-134 LinerMate Accessory.
			5. TA-5: B-2111 ClassicSeries Wall-Mounted Soap Dispenser.
			6. TA-6: KB300-01SS Koala Kare Surface Mount Horizontal Baby Changing Station with Stainless Veneer and External Bag Hook
		2. Single-User Washroom, Heavy Duty:
			1. TA-1: B-6806 Series Concealed Mounting Grab Bar – 1-1/2 inch diameter.
			2. TA-2: B-290 Series Angle-Frame Mirror.
			3. TA-3: B-3888 ClassicSeries Recessed Multi-Roll Toilet Tissue Dispenser.
			4. TA-4: B-3961 ClassicSeries Recessed Touch Free, Pull-Towel, Universal Roll Paper Towel Dispenser and Waste Receptacle with 3944-134 LinerMate Accessory.
			5. TA-5: B-2111 ClassicSeries Wall-Mounted Soap Dispenser.
			6. TA-6: KB310-SSRE Koala Kare Recessed Horizontal Baby Changing Station with External Bag Hook
		3. Single-User Washroom, Premium:
			1. TA-1: B-6806 Series Concealed Mounting Grab Bar – 1-1/2 inch diameter.
			2. TA-1A: B-9806 Fino-Collection Concealed Mounting Grab Bar – 1-1/2 inch diameter.
			3. TA-2: B-290 Series Angle-Frame Mirror.
			4. TA-3: B-4388 ConturaSeries Recessed Multi-Roll Toilet Tissue Dispenser.
			5. TA-3A: B-9547 Fino-Collection Toilet Roll Holder double.
			6. TA-4: B-43944 ConturaSeries Recessed Paper Towel Dispenser / Waste Receptacle with TowelMate and LinerMate.
			7. TA-4A: B-9262 Fino-Collection Surface-Mounted paper towel dispenser with LinerMate.
			8. TA-4B: B-9279 Fino-Collection tiltable Surface-Mounted waste receptacle with leak proof rigid plastic waste container.
			9. TA-4C: B-7179 Fino-Collection Surface-Mounted automatic Hand Dryer.
			10. TA-5: B-828 Automatic, Countertop-Mounted Foam Soap Dispenser.
			11. TA-5A: B-8878 Automatic, Cast Brass Electronic-Sensor Operated Faucet with Polished Chrome Finish

(or)

* + - 1. TA-5B: B-868 Automatic, Counter-Mounted, Die-Cast Zinc Top-Fill Foam Soap Dispenser with Polished Chrome Finish
			2. TA-5C: B-8898 Automatic, Cast Brass Electronic-Sensor Operated Faucet with Polished Chrome Finish
		1. Multiple-Use Washroom, Standard Duty:
			1. TA-1: B-5806 Series Concealed Mounting Grab Bar – 1-1/4 inch diameter.
			2. TA-2: B-165 Series Channel-Frame Mirror.
			3. TA-3: B-2888 ClassicSeries Surface-Mounted Multi-Roll Toilet Tissue Dispenser.
			4. TA-4: B-3944 ClassicSeries Recessed Paper Towel Dispenser / Waste Receptacle with 3944-130 TowelMate Accessory and 3944-134 LinerMate Accessory.

(or)

* + - 1. TA-4A: B-262 ClassicSeries Surface-Mounted Paper Towel Dispenser with 262-130 TowelMate Accessory.
			2. TA-4B: B-279 ClassicSeries Surface-Mounted Waste Receptacle.
			3. TA-4C: B-7128 TrimLine Series Surface-Mounted Automatic Hand Dryer.

(and)

* + - 1. TA-5: B-2111 ClassicSeries Wall-Mounted Soap Dispenser.
			2. TA-6: B-254 ClassicSeries Surface-Mounted Sanitary Napkin Waste Receptacle.
			3. TA-7: B-2706 25 ClassicSeries Surface-Mounted Sanitary Napkin / Tampon Vendor.
			4. TA-8: KB300-01SS Koala Kare Surface-Mounted Horizontal Baby Changing Station with Stainless Veneer and External Bag Hook
		1. Multiple-Use Washroom, Heavy-Duty:
			1. TA-1: B-6806 Series Concealed Mounting Grab Bar – 1-1/2 inch diameter.
			2. TA-2: B-290 Series Angle-Frame Mirror.
			3. TA-3: B-4288 ConturaSeries Surface-Mounted Multi-Roll Toilet Tissue Dispenser.
			4. TA-4: B-3974 ClassicSeries Recessed Automatic, Universal Roll Paper Towel Dispenser and Waste Receptacle with 3944-134 LinerMate Accessory.

(or)

* + - 1. TA-4A: B-2860 Surface-Mounted Touch-Free, Pull-Towel, Universal Roll Paper Towel Dispenser.
			2. TA-4B: B-2250 Floor Standing Swing-Top Waste Receptacle.
			3. TA-4C: B-7125 InstaDry Surface-Mounted High-Speed Hand Dryer.

(and)

* + - 1. TA-5: B-2111 ClassicSeries Wall-Mounted Soap Dispenser.
			2. TA-6: B-354 ClassicSeries Partition-Mounted Sanitary Napkin Waste Receptacle.
			3. TA-7: B-3706 25 ClassicSeries Recessed Sanitary Napkin / Tampon Vendor.
			4. TA-8: KB310-SSRE Koala Kare Recessed Baby Changing Station with External Bag Hook
			5. TA-9: KB102-00 Koala Kare Products Wall-Mounted Child Protection Seat.
		1. Multiple-Use Washroom, Premium:
			1. TA-1: B-6806 Series Concealed Mounting Grab Bar – 1-1/2 inch diameter.
			2. TA-1A: B-9806 Fino-Collection Concealed Mounting Grab Bar – 1-1/2 inch diameter.
			3. TA-2: B-290 Series Angle-Frame Mirror.
			4. TA-3: B-4288 ConturaSeries Surface-Mounted Multi-Roll Toilet Tissue Dispenser.
			5. TA-3A: B-9547 Fino-Collection Toilet Roll Holder double.
			6. TA-4: B-43944 ConturaSeries Recessed Paper Towel Dispenser / Waste Receptacle with TowelMate and LinerMate.

(or)

* + - 1. TA-4A: B-4262 ConturaSeries Surface-Mounted Paper Towel Dispenser with TowelMate.
			2. TA-4B: B-43644 ConturaSeries Recessed Waste Receptacle with LinerMate.
			3. TA-4C: B-3725 Recessed Hand Dryer.
			4. TA-4AA: B-9262 Fino-Collection Surface-Mounted Paper Towel Dispenser with LinerMate.
			5. TA-4BB: B-9279 Fino-Collection tiltable Surface-Mounted Waste Receptacle with leak proof rigid plastic waste container.
			6. TA-4CC: B-7179 Fino-Collection Surface-mounted Automatic Hand Dryer.

(and)

* + - 1. TA-5: B-828 Automatic, Countertop-Mounted Foam Soap Dispenser.
			2. TA-5A: B-8878 Automatic, Cast Brass Electronic-Sensor Operated Faucet with Polished Chrome Finish

(or)

* + - 1. TA-5B: B-868: Automatic, Counter-Mounted, Die-Cast Zinc Top-Fill Foam Soap Dispenser with Polished Chrome Finish
			2. TA-5C: B-8898 Automatic, Cast Brass Electronic-Sensor Operated Faucet with Polished Chrome Finish

(or)

* + - 1. TA-5D: B-820 Automatic, Multi-Feed Soap Dispensing System with 820-248 Automatic Foam Dispenser or 820-258 Automatic Liquid Dispenser.
			2. TA-6: B-270 ConturaSeries Surface-Mounted Sanitary Napkin Waste Receptacle.
			3. TA-7: B-4706 25 ConturaSeries Recessed Sanitary Napkin / Tampon Vendor.
			4. TA-8: TA-6: KB310-SSRE Koala Kare Recessed Baby Changing Station with External Bag Hook
			5. TA-9: KB102-00 Koala Kare Products Wall-Mounted Child Protection Seat.
			6. TA-10: B-4221 ConturaSeries Surface-Mounted Seat Cover Dispenser
1. EXECUTION
	1. INSTALLATION
		1. Install products in strict compliance with manufacturer’s written instructions and recommendations, including the following:
			1. Verify blocking has been installed properly.
			2. Verify location does not interfere with door swings or use of fixtures.
			3. Comply with manufacturer’s recommendations for backing and proper support.
			4. Use fasteners and anchors suitable for substrate and project conditions.
			5. Install units rigid, straight, plumb, and level, in accordance with manufacturer’s installation instructions and approved shop drawings.
			6. Conceal evidence of drilling, cutting, and fitting to room finish.
			7. Test for proper operation.
	2. CLEANING AND PROTECTION
		1. Clean exposed surfaces of compartments, hardware, and fittings using methods acceptable to the manufacturer.
		2. Touch-up, repair or replace damaged products until Substantial Completion.

 END OF SECTION